|  |  |  |  |
| --- | --- | --- | --- |
| To | **ALL** | Doc. No. |  |
| CC |  | Country |  |
| From |  | E-mail |  |
| Subject | **SMT-i601x, SMT-i602x Phone S/W PKG Release** | | |

**S/W release**

|  |  |  |
| --- | --- | --- |
| **System** | **Package name** | **Description** |
| SCM Express  SCM Compact | i6011\_SCME\_V01.40\_20160930.tar.gz  i6021\_SCME\_V01.40\_20160930.tar.gz | WCM V5.4.2~  SCM Compact |

## New Version V01.40 (SMT-60xx supported)

**V01.40 (160930)**

* **New**

|  |  |  |
| --- | --- | --- |
| **No** | **Item** | **description** |
| 1 | Ring Preference | SCM Compact v2.0 |
| 2 | Ring Deflect | SCM Compact v2.0 |
| 3 | Multicast Paging Rejoin | SCM Compact v2.0 |
| 4 | System Info. Display | SCM Compact v2.0 |
| 5 | Nursing Home Service (Emergency Message) | SCM Compact v2.0 |
| 6 | Add “Log Browser” to Engineer-menu | SMT-i60xx |
| 7 | Add operating EHS headset models  Jabra : Jabra BIZ 2300 , Jabra PRO 9470 UK  Sennheisser : Sennheisser SC 70 USB, Sennheisser DW Office  (USB Connection Only available. Analog Connection is not supported) | SMT-i60xx |
| 8 | Add language - French | SCM Compact v2.0 |
| 9 | Restrict to edit/delete program(AOM) key which cannot be created  by phone. | SMT-i60xx |

* **Enhancement**

|  |  |  |
| --- | --- | --- |
| **No** | **항목** | **비고** |
| 1 | Change the BT/EHS headset key operation(hook on) in transfer state  Previous : end current call (cancel outgoing call to transferee)  -> Changed : transfer call to transferee | SMT-i60xx |
| 2 | Fix the issue that peer voice sounds shortly in speaker when user ends  call by using EHS headset key. | SMT-i60xx |
| 3 | Fix the issue about call history redial failure. (inbound call) | SMT-i602x |
| 4 | Fix the issue about USB-Easy setup  - The start-up with a wireless network with hidden SSID fail | SMT-i60xx |
| 5 | Add key order sorting feature with programmable key menu | SMT-i601x |
| 6 | Change the EHS headset key operation(hook off) in idle state  Previous : not happened  -> Change : change to dial state | SMT-i60xx |
| 7 | Add programmable key attribute  Example) ACD break with code | SMT-i60xx |

|  |  |  |  |
| --- | --- | --- | --- |
| To | **ALL** | Doc. No. |  |
| CC |  | Country | **KOR** |
| From |  | E-mail |  |
| Subject | **SMT-i601x, SMT-i602x Phone S/W PKG Release** | | |

**S/W release**

|  |  |  |
| --- | --- | --- |
| **System** | **Package name** | **Description** |
| SCM Express  SCM Compact | i6011\_SCME\_V01.34\_20160712.tar.gz  i6021\_SCME\_V01.34\_20160721.tar.gz | WCM V5.4.2~  SCM Compact |

## New Version V01.34 (SMT-60xx supported)

**V01.34 (160712)**

* **Enhancement**

|  |  |  |
| --- | --- | --- |
| **No** | **Item** | **description** |
| 1 | Fix the invalid string.   * Broken string on message menu title (only V01.33) * Cut string in several languages when displaying “Not supported” | SMT-i601x |

|  |  |  |  |
| --- | --- | --- | --- |
| To | **ALL** | Doc. No. |  |
| CC |  | Country | **KOR** |
| From |  | E-mail |  |
| Subject | **SMT-i601x, SMT-i602x Phone S/W PKG Release** | | |

**S/W release**

|  |  |  |
| --- | --- | --- |
| **System** | **Package name** | **Description** |
| SCM Express  SCM Compact | i6011\_SCME\_V01.33\_20160705.tar.gz  i6021\_SCME\_V01.33\_20160705.tar.gz | WCM V5.4.2~  SCM Compact |

## New Version V01.33 (SMT-60xx supported)

**V01.33 (160705)**

* **Enhancement**

|  |  |  |
| --- | --- | --- |
| **No** | **Item** | **description** |
| 1 | Reduce echo during phone recording service | SMT-i60xx |
| 2 | Modify volume level of EHS headset (volume up) | SMT-i60xx |
| 3 | Fix the time freezing issue of SMT-i601x with ping-ring service | SMT-i601x |
| 4 | Modify incorrect language display – Dutch, Italian | SMT-i60xx |
| 5 | Fix the issue from Italy.  - Displaying broken boot up screen with USB easy install – SMT-i601x | SMT-i601x |

|  |  |  |  |
| --- | --- | --- | --- |
| To | **ALL** | Doc. No. |  |
| CC |  | Country | **KOR** |
| From |  | E-mail |  |
| Subject | **SMT-i601x, SMT-i602x Phone S/W PKG Release** | | |

**S/W release**

|  |  |  |
| --- | --- | --- |
| **System** | **Package name** | **Description** |
| SCM Express | i6011\_SCME\_V01.30\_20160427.tar.gz  i6021\_SCME\_V01.30\_20160427.tar.gz | WCM V5.4.2  SCM Compact v2 (Dutch, Swedish) |

## New Version V01.30 (SMT-60X0 supported)

**V01.30 (160427)**

* **New**

|  |  |  |
| --- | --- | --- |
| **No** | **Item** | **description** |
| 1 | Enable to set phone password in WCM | WCM v5.4.2 |
| 2 | Enable to set the option, “Use Hardware Headset Key” in WCM | WCM v5.4.2 |
| 3 | Enable to set allowance the Web-access in WCM | WCM v5.4.2 |
| 4 | Multicast Paging | WCM v5.4.2 |
| 5 | Enable to set allowance the use of PC-VLAN in WCM | WCM v5.4.2 |
| 6 | Add language – Dutch, Swedish | SCM Compact v2.0 |

* **Enhancement**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **No** | | **Item** | | | **description** | |
| 1 | | Block next consecutive outgoing call without previous call response  from server | | |  | |
| 2 | | OpenSSL Version Up | | | OpenSSL 1.0.1p -> 1.0.1r | |
| 3 | | Change the method to read default password  Hard-coded in source -> Read value from encrypted file | | |  | |
| 4 | | Reduce periodically occurred noise with EHS headset | | |  | |
| 5 | | Bug fixed for the change of network speed  (Phone intermittently changed the network speed to 10/half.) | | |  | |
| 6 | | Bug fixed for displaying caller name with “Anonymous” in call history  above the count 300 | | | SMT-i601x | |
| 7 | | Volume control GUI changed | | | SMT-i602x | |
| 8 | | Bug fixed for reading 802.1x authentication(MD5) password  (Issue occurred when the encrypted password includes the char ‘/’) | | |  | |
| To | | **ALL** | | Doc. No. |  | |
| CC | |  | | Country | **KOR** | |
| From | |  | | E-mail |  | |
| Subject | | **SMT-i601x, SMT-i602x Phone S/W PKG Release** | | | | |

**S/W release**

|  |  |  |
| --- | --- | --- |
| **System** | **Package name** | **Description** |
| SCM Express | i6011\_SCME\_V01.19\_20151016.tar.gz  i6021\_SCME\_V01.19\_20151016.tar.gz | WCM V5.3/V5.4 |

## New Version V01.19 (SMT-60X0 supported)

**V01.19 (151016)**

1. PA Issue Fixed

* AOM communication problem with phone fixed.

: In wired mode and V01.17, If AOM connected to PC port of Phone, It cannot communicate with the phone.

* Keytone volume level problem fixed.
* It supports delimiter ‘;’ when parsing a CVS file for USB Easysetup.

1. DNS query Issue Fixed
   * + In Static IP mode, Phone can’t send DNS query using user setting value.
2. New Feature

Multi language feature added. (Russia, Turkey, Italy)

* Below Issues from Italy has been fixed
  + - [602X] Alphabetic entry mode during numerical search
    - [602X] Date and Time text translated in idle display
    - [602X] Wrong string displayed (Program Key configurations)
    - [602X] Duplicated symbol backspace (Program Key configurations)
    - [602X] Wrong string in the call service
    - [601X] Issues has been applied in the Roberto’s email
    - [601X] Broken Softmenu guide line

**S/W release**

|  |  |  |
| --- | --- | --- |
| **System** | **Package name** | **Description** |
| SCM Express | i6011\_SCME\_V01.17\_20150909.tar.gz  i6021\_SCME\_V01.17\_20150909.tar.gz | WCM V5.3/V5.4 |

## New Version V01.17 (SMT-60X0 supported) – PRA

**V01.17 (150909)**

1. New Feature

USB Easy-install feature added.

1. PA Issue Fixed

**S/W release**

|  |  |  |
| --- | --- | --- |
| **System** | **Package name** | **Description** |
| SCM Express | i6011\_SCME\_V01.16\_20150907.tar.gz  i6021\_SCME\_V01.16\_20150907.tar.gz | WCM V5.3/V5.4 |

## New Version V01.16 (SMT-60X0 supported)

**V01.16 (150907)**

1. PA Issue Fixed.

**S/W release**

|  |  |  |
| --- | --- | --- |
| **System** | **Package name** | **Description** |
| SCM Express | i6011\_SCME\_V01.15\_20150901.tar.gz  i6021\_SCME\_V01.15\_20150901.tar.gz | WCM V5.3/V5.4 |

## New Version V01.15 (SMT-60X0 supported)

**V01.15 (150901)**

1. PA Issue Fixed.
   * + A History button of SMT-i602X model is moved from 2nd to 3rd button on Idle display.
     + SMT-i601X model supports a feature MMC 109 (Date format)
2. SEA Issue Fixed
   * + Issue about updating DNS address from DHCP server is fixed.

**S/W release**

|  |  |  |
| --- | --- | --- |
| **System** | **Package name** | **Description** |
| SCM Express | i6011\_SCME\_V01.14\_20150818.tar.gz  i6021\_SCME\_V01.14\_20150818.tar.gz | WCM V5.3/V5.4 |

## New Version V01.14 (SMT-60X0 supported)

**V01.14 (150818)**

1. New Features
   1. OpenSSL version up (1.0.1h -> 1.0.1p)
   2. Auto Answer icon indicator added (SMT-i602X, WCM)
   3. USB Easysetup function added.
2. PA Issue Fixed.

|  |  |  |  |
| --- | --- | --- | --- |
| To | **ALL** | Doc. No. |  |
| CC |  | Country | **KOR** |
| From |  | E-mail |  |
| Subject | **SMT-i601x, SMT-i602x Phone S/W PKG Release** | | |

**Overview:**

**S/W release**

|  |  |  |
| --- | --- | --- |
| **System** | **Package name** | **Description** |
| SCM Express | i6011\_SCME\_V01.13\_20150803.tar.gz  i6021\_SCME\_V01.13\_20150803.tar.gz | WCM V5.3 |

## New Version V01.13 (SMT-60X0 supported)

**V01.13 (150803)**

\* Supports both SMT-i60X1 and SMT-i60X0 models.

1. SMT-i60x1 s/w PA patch released

- PA issue fixed.

- Issue fixed VLAN failure without LLDP (Sometimes).

- New Feature added.

. Personal Web Management (WCM only)

User can access the phone with web browser on the PC.

*http://phone\_IP:8080*, (admin/samsung\*# or user/samsung)

(Higher then IE 9.0 or Google Chrome browser is recommended.)

|  |  |  |  |
| --- | --- | --- | --- |
| To | **ALL** | Doc. No. |  |
| CC |  | Country | **KOR** |
| From |  | E-mail |  |
| Subject | **SMT-i6011, SMT-i6021 Phone S/W PKG Release** | | |

**Overview:**

**S/W release**

|  |  |  |
| --- | --- | --- |
| **System** | **Package name** | **Description** |
| SCM Express | i6011\_SCME\_V01.11\_20150623.tar.gz  i6021\_SCME\_V01.11\_20150623.tar.gz | WCM V5.3 |

## New Version V01.11

**V01.11 (150623)**

1. SMT-i60x1 s/w PA patch released

- STA Lab. test issue fixed.

1) Issue fixed USB Upgrade failure (Sometimes).

2) 60x1 phone’s dial tone volume level is adjusted

|  |  |  |  |
| --- | --- | --- | --- |
| To | **ALL** | Doc. No. |  |
| CC |  | Country | **KOR** |
| From |  | E-mail |  |
| Subject | **SMT-i6011, SMT-i6021 Phone S/W PKG Release** | | |

**Overview:**

**S/W release**

|  |  |  |
| --- | --- | --- |
| **System** | **Package name** | **Description** |
| SCM Express | i6011\_SCME\_V01.10\_20150615.tar.gz  i6021\_SCME\_V01.10\_20150615.tar.gz | WCM V5.3 |

## New Version V01.10

**V01.10 (150615)**

1. SMT-i60x1 s/w PA patch released

- STA Lab. test issue fixed.

1) Can’t display external caller name and number at the same time.

|  |  |  |  |
| --- | --- | --- | --- |
| To | **ALL** | Doc. No. |  |
| CC |  | Country | **KOR** |
| From |  | E-mail |  |
| Subject | **SMT-i6011, SMT-i6021 Phone S/W PKG Release** | | |

**Overview:**

**S/W release**

|  |  |  |
| --- | --- | --- |
| **System** | **Package name** | **Description** |
| SCM Express | i6011\_SCME\_V01.09\_20150608.tar.gz  i6021\_SCME\_V01.09\_20150608.tar.gz | WCM V5.3 |

## New Version V01.09

**V01.09 (150608)**

1. SMT-i60x1 s/w PA patch released

- STA Lab. test issue fixed.

1) Red LED on top of the phone (TSI) is slow to turn on after a new message is left in the voice mail box. About 5 seconds.

2) Display message is changed

“Logout” -> “Logged Out”

“Now Login” -> “Now Logging In”

3) After dialing the Logout codes \*99 the display shows the user ID and Password of the last user.

- SEUK Lab. Test issue fixed.

1) On the handset, after completing setup of Bluetooth headset and at the point of searching for the headset, the screen prompt reads 'Research'. Should read 'Search'.

- PA issue fixed

1) [6021] WIFI status icon images are changed in the setting menu.

2) [6011] SRTP call status icon is changed.

|  |  |  |  |
| --- | --- | --- | --- |
| To | **ALL** | Doc. No. |  |
| CC |  | Country | **KOR** |
| From |  | E-mail |  |
| Subject | **SMT-i6011, SMT-i6021 Phone S/W PKG Release** | | |

**Overview:**

**S/W release**

|  |  |  |
| --- | --- | --- |
| **System** | **Package name** | **Description** |
| SCM Express | i6011\_SCME\_V01.08\_20150527.tar.gz  i6021\_SCME\_V01.08\_20150527.tar.gz | WCM V5.3 |

## New Version V01.08

**V01.08 (150527)**

1. SMT-i60x1 검증 5차 패치

- 검증 이슈 수정

PA, 신뢰성/제품기술 문제점 수정

|  |  |  |  |
| --- | --- | --- | --- |
| To | **ALL** | Doc. No. |  |
| CC |  | Country | **KOR** |
| From |  | E-mail |  |
| Subject | **SMT-i6011, SMT-i6021 Phone S/W PKG Release** | | |

**Overview:**

**S/W release**

|  |  |  |
| --- | --- | --- |
| **System** | **Package name** | **Description** |
| SCM Express | i6011\_SCME\_V01.07\_20150526.tar.gz  i6021\_SCME\_V01.07\_20150526.tar.gz | WCM V5.3 |

## New Version V01.07

**V01.07 (150526)**

1. SMT-i60x1 검증 4차 패치

- 검증 이슈 수정

PA, 신뢰성/제품기술 문제점 수정

|  |  |  |  |
| --- | --- | --- | --- |
| To | **ALL** | Doc. No. |  |
| CC |  | Country | **KOR** |
| From |  | E-mail |  |
| Subject | **SMT-i6011, SMT-i6021 Phone S/W PKG Release** | | |

**Overview:**

**S/W release**

|  |  |  |
| --- | --- | --- |
| **System** | **Package name** | **Description** |
| SCM Express | i6011\_SCME\_V01.05\_20150518.tar.gz  i6021\_SCME\_V01.05\_20150518.tar.gz | WCM V5.3 |

## New Version V01.05

**V01.05 (150518)**

1. SMT-i60x1 검증 3차 패치

- 검증 이슈 수정

PA, 신뢰성/제품기술 문제점 수정

|  |  |  |  |
| --- | --- | --- | --- |
| To | **ALL** | Doc. No. |  |
| CC |  | Country | **KOR** |
| From |  | E-mail |  |
| Subject | **SMT-i6011, SMT-i6021 Phone S/W PKG Release** | | |

**Overview:**

**S/W release**

|  |  |  |
| --- | --- | --- |
| **System** | **Package name** | **Description** |
| SCM Express | i6011\_SCME\_V01.04\_20150508.tar.gz  i6021\_SCME\_V01.04\_20150508.tar.gz | WCM V5.3 |

## New Version V01.04

**V01.04 (150508)**

1. SMT-i60x1 검증 2차 패치
   1. 미구현 기능 구현

- USB를 통한 SDM 연동 기능

(VQMON은 9월 버전에 포함하기로 협의)

2. 검증 이슈 수정

|  |  |  |  |
| --- | --- | --- | --- |
| To | **ALL** | Doc. No. |  |
| CC |  | Country | **KOR** |
| From |  | E-mail |  |
| Subject | **SMT-i6011, SMT-i6021 Phone S/W PKG Release** | | |

**Overview:**

**S/W release**

|  |  |  |
| --- | --- | --- |
| **System** | **Package name** | **Description** |
| SCM Express | i6011\_SCME\_V01.02\_20150420.tar.gz  i6021\_SCME\_V01.02\_20150420.tar.gz | WCM V5.3 |

## New Version V01.02

**V01.02 (150420)**

1. SMT-i60x1 검증 1차 패치
   1. 미구현 기능 구현

- KT Loopback 기능

- EHS Headset 연동

- Wave Key Tone 재생기능

- Syslog 기능 (시스템 연동)

- Hook On/Off Timer (단말 기본 Timer 값만 적용, 시스템 구현 및 시험 중)

* 1. 검증 이슈 수정

|  |  |  |  |
| --- | --- | --- | --- |
| To | **ALL** | Doc. No. |  |
| CC |  | Country | **KOR** |
| From |  | E-mail |  |
| Subject | **SMT-i6011, SMT-i6021 Phone S/W PKG Release** | | |

**Overview:**

**S/W release**

|  |  |  |
| --- | --- | --- |
| **System** | **Package name** | **Description** |
| SCM Express | i6011\_SCME\_V01.00\_20150406.tar.gz  i6021\_SCME\_V01.00\_20150406.tar.gz | WCM V5.3 |

## New Version V01.00

**V01.00 (150406)**

1. SMT-i60x1(New Design Wireless IP Phone 과제) 최초 PA 의뢰버전